**General:** Lockers shall be " Recruiter Wood Sport Lockers" as manufactured by Hallowell or approved equal. All lockers shall be factory-assembled

**Finish:** All locker parts to be finished with Two-coat formaldehyde-free conversion clear varnish finish (or equivalent).

**Locker Body:** Constructed from 3/4" plain sliced red oak plywood with hardwood and wood veneer throughout. This includes the security lockbox door, sides, footlocker grates, seats, and upper/lower shelves. The back and bottom panels will also be 3/4" plain sliced red oak plywood

**Locker Trim:** Face trim, shelf valances, personal effects locker doors, seat front nosing, hinge support blocking, and seat support cleats will be fabricated from red oak plywood with wood edge banding (no PVC edging allowed).

**Upper Shelf:** Constructed from 3/4" red oak plain sliced plywood.

**Standard Hardware:** Includes three single-prong stainless steel coat hooks, a KV 1 1/16" diameter stainless steel clothes hanging rod with .075" wall thickness, and European soft-close hinges for the upper security box door.

**Locks (If required):** Standard options include a chrome padlock hasp or a Master Lock 1655 built-in combination lock.

**Stock Sizes:** 24" wide x 24" deep x 84" high 30" wide x 24" deep x 84" high

**One Year Warranty:** Superior Recruiter Lockers are covered against all defects in materials and workmanship excluding finish, damage resulting from deliberate destruction and vandalism under this section for a period of one year.